{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["EDM SO BW Return 2024"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EDM SO BW Return 2024","index":0,"n_rows":5,"n_cols":24,"rows_kept":5,"cut":false,"hidden":false,"merged":[[1,19,2,20],[1,12,2,12]]}
["EDM STORM OVERFLOW REGULATORY RETURN - BATHING WATER SEASON"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select names from drop down, multiple can be selected",null,null,null,null,null,null,"Complete columns T & U when data in column S is <90%"]
[]
["Unique ID","Water Company Name","Site Name\n(EA Consents Database)","Site Name\n(WaSC operational)\n[optional]","EA Permit Reference\n(EA Consents Database)","WaSC Supplementary Permit Ref.\n[optional]","Activity Reference on Permit","Storm Discharge Asset Type","Outlet Discharge NGR\n(EA Consents Database)","WFD Waterbody ID (Cycle 3)\n(discharge outlet)","WFD Waterbody Catchment Name (Cycle 3)\n(discharge outlet)","Receiving Water / Environment (common name)\n(EA Consents Database)","Bathing Water Name(s)","Bathing Water Type","Treatment Method on Permit\n(over & above Storm Tank settlement / screening)","Initial EDM Commission Date","Total Duration (hrs) all spills prior to processing through 12-24h count method","Counted spills using 12-24h count method","EDM Operation -\n% of reporting period EDM operational","EDM Operation -\nReporting % -\nPrimary Reason <90%","EDM Operation -\nAction taken / planned -\nStatus & timeframe","Previous Improvements -\nMost recent AMP period asset previously improved\n(under BW WINEP driver)","Target Standard affecting Spill Frequency\n(if SO previously improved)","Spill Frequency for Design Solution\n(significant spills)\n(if SO previously improved)"]
["AnW1345","Anglian Water","NEWTON MARSH WATER RECYCLING CENTRE","TETNEY-NEWTON MARSH STW","ANNTS13007","ANNTS13007/V001","A2","Storm tank at WwTW","TA3543003200","GB530402609201","Waithe Beck lower catchment (to Tetney Lock) Water Body","Tetney Haven","Cleethorpes, Humberston Fitties","Coastal","N/A","Commissioned in 2018 - full BW season data expected",16.399999999999999,19,1,null,null,"N/A","N/A","N/A"]